send/receive send/receive 0 50 100 150 200 250 300 350 400 450 overhead in iWarp clock cycles (@50ns) synch. switch (software) msg-setup (route gen.+hardware set) DMA (spooler) setup propagation in netw.